**Table S1.**

|  |  |  |
| --- | --- | --- |
| **Needle size used to generate holes in parafilm** | **Average ratio between minor and major axes of the generated ellipse hole** | **Standard deviation** |
| 30G | 0.982 | 0.063 |
| 26G | 0.985 | 0.050 |