|  |  |
| --- | --- |
| K | 31 |
| no. of reads used for assembly | N/A |
| no. and % reads not used or assembly | N/A |
| total no .of contigs | 59859 |
| total length of contigs | 19,442,767bp |
| avg length of contigs | 324.8bp |
| longest contig | 7624 |
| no. of contigs equal or greater 100 bp | 54123 |
| total length contigs equal or greater 100 bp | 18,913,114bp |
| avg length of contigs equal or greater 100 bp | 349.5bp |
| N50 for contigs equal or greater 100 bp | 466 |