

**Figure S2.** Mean (+S.E.) metal and total PAH concentrations (dw), sediment Chl-a, TOC, porewater ammonia and percent fines (<63 µm) analysed from benthic sediment grabs collected in heavily modified (filled bars) and relatively unmodified (open bars) estuaries.